COMMANDS

Breeze:

en

conf t

int f3/0

ip address 192.0.24.1 255.255.252.0

no shutdown

int s0/0

ip address 192.0.32.25 255.255.255.248

no shutdown

int s1/0

ip address 192.0.32.33 255.255.255.248

no shutdown

show ip interface brief

Breeze>en

Breeze#conf t

Breeze(config)#ip route 192.0.20.0 255.255.252.0 s0/0

Breeze(config)#ip route 192.0.16.0 255.255.252.0 s0/0

Breeze(config)#ip route 192.0.8.0 255.255.248.0 s1/0

Breeze(config)#ip route 192.0.8.0 255.255.248.0 s0/0 5

Breeze(config)#ip route 192.0.0.0 255.255.248.0 s0/0

Breeze(config)#ip route 192.0.32.0 255.255.252.0 s0/0

Haven:

en

conf t

hostname Haven

int f3/0

ip address 192.0.0.1 255.255.248.0

no shutdown

int s4/0

ip address 192.0.32.9 255.255.255.248

no shutdown

int s0/0

ip address 192.0.32.2 255.255.255.248

no shutdown

en

config t

router rip

version 2

no auto-summary

network 192.0.32.0

network 192.0.32.8

network 192.0.0.0

passive-interface f3/0

exit

end

copy run start

Fracture:

en

conf t

hostname Fracture

int f3/0

ip address 192.0.8.1 255.255.248.0

no shutdown

int s0/0

ip address 192.0.32.41 255.255.255.248

no shutdown

en

config t

router rip

version 2

no auto-summary

network 192.0.32.40

network 192.0.8.0

passive-interface f3/0

exit

end

copy run start

Icebox :

en

conf t

hostname Icebox

int f3/0

ip address 192.0.20.1 255.255.252.0

no shutdown

int s0/0

ip address 192.0.32.26 255.255.255.248

no shutdown

int s1/0

ip address 192.0.32.17 255.255.255.248

no shutdown

Icebox>en

Icebox#conf t

Icebox(config)#ip route 192.0.24.0 255.255.252.0 s0/0

Icebox(config)#ip route 192.0.16.0 255.255.252.0 s1/0

Ascent:

Router>

Router>en

Router#conf t

Router(config)#hostname Ascent

Ascent(config)#int f3/0

Ascent(config-if)#ip address 192.0.16.1 255.255.252.0

Ascent(config-if)#no shutdown

Ascent(config-if)#int s1/0

Ascent(config-if)#ip address 192.0.32.18 255.255.255.248

Ascent(config-if)#no shutdown

Ascent(config-if)#int s0/0

Ascent(config-if)#ip address 192.0.32.42 255.255.255.248

Ascent(config-if)#no shutdown

Ascent(config-if)#int s5/0

Ascent(config-if)#ip address 192.0.32.34 255.255.255.248

Ascent(config-if)#no shutdown

Ascent(config-if)#int s4/0

Ascent(config-if)#ip address 192.0.32.10 255.255.255.248

Ascent(config-if)#no shutdown

Ascent(config-if)#exit

Ascent(config)#ip route 192.0.28.0 255.255.252.0 s4/0

Ascent(config)#ip route 192.0.24.0 255.255.252.0 s5/0

Ascent(config)#ip route 192.0.20.0 255.255.252.0 s1/0

Bind:

Router>en

Router#conf t

Router(config)#hostname Bind

Bind(config)#int f3/0

Bind(config-if)#ip address 192.0.28.1 255.255.252.0

Bind(config-if)#no shutdown

Bind(config-if)#int s1/0

Bind(config-if)#ip address 192.0.32.1 255.255.255.248

Bind(config-if)#no shutdown

en

config t

router rip

version 2

no auto-summary

network 192.0.32.0

network 192.0.28.0

passive-interface f3/0

exit

end

copy run start